                                                               PAGE   2                                                                                         
       This is a explanation of the keys of the MENU screen:
       ----------------------------------------------------------------
       (any key) = DSK#.LOAD
          
        While the screen shows menu RXB is selected pressing 
       any key will be the drive that DSK#.LOAD will be run from.     
       RAMDISK number keys 1 to 9 or the alpha keys A to z.
        Pressing 0 (zero) key will run WDS1.LOAD
         
       ----------------------------------------------------------------
       (ENTER key) = DSK#.UTIL1
          
        While the screen shows menu RXB is selected pressing
       ENTER key allows Assembly Programs to be used. Pressing 
       any key will be the drive that DSK#.UTIL1 will be run from.     
       RAMDISK number keys 1 to 9 or the alpha keys A to z.
        Pressing 0 (zero) key will run WDS1.UTIL1
                   
       --------------------------------------------------------------- 
       (COMMA) , = DSK#.BATCH
          
         While the screen shows menu RXB is selected pressing
       COMMA key runs DSK#.BATCH 
       DSK#.BATCH defaults to DSK1 if BATCH not found will default to 
       command mode. For more information on this feature read USER in 
       the RXB information on BATCH FILE SYSTEM below.

       ----------------------------------------------------------------
       (SPACE BAR) = RXB COMMAND MODE
          
        Pressing the SPACE BAR results in XB command mode.
        (Same as waiting a few seconds just like normal XB does.)

       ----------------------------------------------------------------- 
       (PERIOD) . = EDITOR ASSEMBLER
          
        Pressing the . (PERIOD) key will switch to EDITOR ASSEMBLER
       menu. Pressing the . 

       -----------------------------------------------------------------
       (ZERO) 0 = WSD1.LOAD

         Pressing the 0 (ZERO) key will start a WSD1.LOAD to execute
        from hard drive 1. If the root directory has a LOAD program.