CopyQM converter:


This tools able to convert a CopyQM disk image file to a Raw image usable in Vb81 XuR.

To Do to retrive an image disk:
1) Launch CopyQm using the batch command : "copyqm.exe a: record=MyDisk.CQM BLIND NOSQUEEZE"
2) Use CopyQM manager to convert it in a raw image.

To Do to create an new diskette :
1) You had to retrive the header of you owne diskettes in a CQM file created using an origial disk formated on your ZX81 disk controler.
2) Extract the header using CopyQM converter (a "Header_1.bin" file will be created).
3) Use the bottom caption to creat a CQM file
4) Write your CopyQm image file using : "copyqm.exe a: playback=MyDisk.CQM BLIND" 

Note: 
A) The "Header_1.bin" is a wrong format! It's a 1.44Mb disk format...
B) In case of Double density 3"5 inchs disk, you can take High density disks and put a rubber tape on the left hole (inlay face), the right hole is the Read-Only hole... using a little black cursor.
   Your drive will get the 720kb format instead of 1.44Mb disk and will initialize it in double density format.  

XavSnap.