## ROLC = Rotate Left through Carry

Hex | Mnemonic | Cycles
--- | --- | ---
CE 90 | ROLC A | 12
CE 91 | ROLC B | 12
CE 92 nn | ROLC [N+#nn] | 20
CE 93 | ROLC [HL] | 16

### Execute

    A       = Register A
    B       = Register B
    [N+#nn] = Memory: (I shl 16) or (N shl 8) or #nn
    [HL]    = Memory: (I shl 16) or HL

    ; ROLC Ds
    ;
    ; Ds = Source/Destination

    Ds = (Ds SHL 1) OR Carry

### Description

"8-Bits Destination" bits are rotated left by 1 through Carry.

### Conditions

Zero: Set when result is 0

Carry: Set when old bit 7 is 1

Sign: Set when bit 7 of the result is 1

Overflow remain unchanged

### Examples

    ; A = 0x04
    ; F = (Carry=0)
    ROLC A
    ; A = 0x08
    ; F = (Zero=0):(Carry=0):(Sign=0)

    ; B = 0x45
    ; F = (Carry=1)
    ROLC B
    ; B = 0x8B
    ; F = (Zero=0):(Carry=0):(Sign=1)

    ; B = 0x84
    ; F = (Carry=0)
    ROLC B
    ; B = 0x08
    ; F = (Zero=0):(Carry=1):(Sign=0)

    ; [HL] = 0x80
    ; F = (Carry=0)
    ROLC [HL]
    ; [HL] = 0x00
    ; F = (Zero=1):(Carry=1):(Sign=0)

    ; [HL] = 0x80
    ; F = (Carry=1)
    ROLC [HL]
    ; [HL] = 0x01
    ; F = (Zero=0):(Carry=1):(Sign=0)

« Back to Instruction set

Retrieved from "http://wiki.sublab.net/index.php/PM_Opc_ROLC"

© 2011-2015 by JustBurn - Hardware documentation copy from Sublab by Team-Pokémé