# Information

To include real BIOS, place "bios.min" on the emulator's directory.
When no "bios.min" is present, emulator will use Pokemon-Mini FreeBIOS.

## Supported multicarts

Type 0 - Disabled (Commercial, Prototype)
Read only

Type 1 - Normal 512KB Flash (AM29LV040B)
Read, Erase, Write, Banking and Manufacturer ID

Type 2 - Lupin's 512KB Flash (AM29LV040B)
Read, Erase, Write, Banking and Manufacturer ID

## Keys

### Debugger, SDL & Win32 Platforms

Default Keys:

Pokémon-Mini | PC Keys
--- | ---
D-PAD Left | Arrow Left
D-PAD Right | Arrow Right
D-PAD Up | Arrow Up
D-PAD Down | Arrow Down
Key A | Keyboard X
Key B | Keyboard Z
Key C | Keyboard S or C
Power Button | Keyboard E
Shock Detector | Keyboard A
UI Menu | Keyboard Esc

F9 will capture the screen and save as "snap_(sequence number).bmp"

F10 can toggle between Fullscreen and Windowed.

F11 will disable/enable speed throttle

TAB can be hold to temporary disable speed throttle

### NDS - Nintendo DS

Default Keys:

Pokémon-Mini | NDS Keys
--- | ---
D-PAD Left | D-PAD Left
D-PAD Right | D-PAD Right
D-PAD Up | D-PAD Up
D-PAD Down | D-PAD Down
Key A | Key A
Key B | Key B
Key C | Shoulder R
Power Button | Start
Shock Detector | Shoulder L
UI Menu | Select

### PSP - PlayStation Portable

Default Keys:

Pokémon-Mini | PSP Keys
--- | ---
D-PAD Left | D-PAD Left
D-PAD Right | D-PAD Right
D-PAD Up | D-PAD Up
D-PAD Down | D-PAD Down
Key A | Circle
Key B | Cross
Key C | Shoulder R
Power Button | Start
Shock Detector | Shoulder L
UI Menu | Select

### WIZ - GP2x Wiz

Default Keys:

Pokémon-Mini | Wiz Keys
--- | ---
D-PAD Left | D-PAD Left
D-PAD Right | D-PAD Right
D-PAD Up | D-PAD Up
D-PAD Down | D-PAD Down
Key A | Key B
Key B | Key X
Key C | Shoulder R
Power Button | Select
Shock Detector | Shoulder L
UI Menu | Menu

### DC - Dreamcast

Default Keys:

Pokémon-Mini | DC Keys
--- | ---
D-PAD Left | D-PAD Left or Joystick
D-PAD Right | D-PAD Right or Joystick
D-PAD Up | D-PAD Up or Joystick
D-PAD Down | D-PAD Down or Joystick
Key A | Key B
Key B | Key A
Key C | Shoulder R
Power Button | Start
Shock Detector | Shoulder L
UI Menu | Key X

### Dingux - Dingoo in Linux

Default Keys:

Pokémon-Mini | Dingoo Keys
--- | ---
D-PAD Left | D-PAD Left
D-PAD Right | D-PAD Right
D-PAD Up | D-PAD Up
D-PAD Down | D-PAD Down
Key A | Key A
Key B | Key B
Key C | Shoulder R
Power Button | Start
Shock Detector | Shoulder L
UI Menu | Select

© 2011-2015 by JustBurn - Hardware documentation copy from Sublab by Team-Pokémé